

**iWiscloud Smart Control Box**

**Operating Manual**

**http://www.iwiscloud.com**



**【Warning】**

iWiscloud smart control box should be installed by qualified electrician and used in accordance with appropriate codes and regulation. Please do not attempt to dismantle this delicate product, willful manipulation might lead to electrical failure. Warranty will be void if product is found to be tampered with.

【**Disclaimer**】：

There might be discrepancies with this manual and the actual product received as our product is constantly being improved upon. Please go to http://[en.iwiscloud.com](http://www.iwiscloud.com) to download the latest product manual. This product is only to be used as intended and any misuse will void the warranty of the product.

**1、 Product Introduction：**

Wiscloud is grateful for your choice to purchase our iWiscloud smart control box. For your safety and maximizing our product capabilities, we would highly encourage you to study this operation manual in details and safe keep for future reference.


**1.1 Key Features：**

* Powerful through-wall ability, its cover is ABS Non-flammable material, simple installation;
* Can be used to pair with 2.4Ghz remote control devices, no re-wiring necessary;

**1.2 Function**

iWiscloud Smart Control Box can pair with 10 switches.


**1.3 Product Wiring Diagram**

****

**Red：Live Blue：Neutral Yellow：Load**

**1.4 Installation Steps**

iWiscloud Smart Control Box (Small):

****

**Note: After connecting Live and Neutral lines, can pair with 2.4GHz devices.**

2、 Product Specifications

|  |  |
| --- | --- |
| Specification | iWiscloud Smart Control Box |
| Rated Power： | 3000W |
| Dimension： | 98mm\*40mm\*23mm |
| Operating Voltage: | 100V~240V AC 50\60Hz  Name |
| Energy Consumption： | <0.5W |
| Lifespan： | ≥ 100,000 times at 220V operating voltage |
| Installation Limitation： | It cannot be installed in a metal shield and magnetic interference place |
| Working Temperature： | -25℃ - 70℃ |
| Cover Material： | PC Non-flammable material |
| Transmission Frequency： | 2.4GHz |

3、 Pairing Methods

It’s necessary to touch the black button to turn on/off smart control box.

3.1 Pairing: Press & hold the black button, after listening to one beep sound then press the paired switch/ remote controller /iWiscloud smart home control center quickly;

3.2 Clear pairing: Press & hold the black button, after listening to three beep sounds to show the pairing has been deleted.

4、Customer Service and Warranty

Yantai Wiscloud Cloud Computing Co., Ltd. provides the following national warranty coverage for iWiscloud smart home control center:

1. If there is performance failure, customers can return, exchange or repair products within 7 days from the date of original retail purchase.

2. If there is performance failure, customers can exchange or repair products within 15 days from the date of original retail purchase.

3. 12 months warranty covered from the date of original retail purchase, but the parts warranty are not covered.

4、iWiscloud Smart Control Box is warranted for the specified Warranty Period from the date of original retail purchase against defects in quality and materials under normal, non-commercial use. Abnormal usage caused damage is not warranty covered. Abnormal usage includes (force majeure), but limited to, deliberate damaging, disassembling, dismantle, manipulating warranty stick, power overloading, water damaging or other man-made caused product damages.

5、Product Checklist

|  |  |
| --- | --- |
| Items | Quantity |
| iWiscloud Smart Control Box | 1 |
| Instruction Manual | 1 |
| Self-tapping Screws | 2 |
| Plastic Bolts | 2 |
| Warranty Card | 1 |
| Quality Control Certificate | 1 |

**6、Company Information**

URL: http://en.iwiscloud.com

E-mail：[service@iwiscloud.com](mailto:service@iwiscloud.com)

**Yantai Wiscloud Cloud Computing Co., Ltd. reserves its right in the terms and conditions interpretation found within this operational manual.**