



**iWiscloud® Smart Dimmer Switch**

# US Edition

**Operating Manual**

**http://www.iwiscloud.com**

**【Warning】：**

iWiscloud smart dimmer switch should be installed by qualified electrician and used in accordance with appropriate codes and regulation. Please do not attempt to dismantle this delicate product, willful manipulation might lead to electrical failure. Warranty will be void if product be found to be tampered with.

【**Disclaimer**】：

There might be discrepancies with this manual and the actual product received as our product is constantly being improved upon. Please go to http://[en.iwiscloud.com](http://www.iwiscloud.com) to download the latest product manual. This product is only to be used as intended and any misuse will void the warranty of the product.

1. **Product Introduction：**

Wiscloud is grateful for your choice to purchase our iWiscloud smart dimmer switch. For your safety and maximizing our product capabilities, we would highly encourage you to study this operation manual in details and safe keep for future reference.

**1.1 Key Features：**

* Pairing with iWiscloud Smart Home Control Center:
* Based on propriety Nebula Protocol, can achieve multi-level floors control;
* Intrinsic safety designed switch features spark-less, over-voltage & over-heating prevention measures;
* Tempered glass panel facade design;

Stylish and safe;

High reliability and stability;


Insulation for “wet hands” operation;

Reactive touch button sensor;

* Simple installation, no re-wiring necessary;
* Current feedback & failure detection;

This product had been designed and manufactured in accordance to strict International safety standards and achieved CE certifications.

**1.2 Product Wiring Diagram**




**Red：Live Blue：Neutral Yellow：Load**

(1)One-gang switch terminal ports：

|  |  |  |
| --- | --- | --- |
| L：power port，Live | N ：power port，Neutral | L2：Load |

**1.3 Installation Steps：**

****

**2、 Product Specifications：**

**BTA Version**

|  |  |
| --- | --- |
| Operating Voltage： | 100~240VAC 50\60Hz |
| Current： | ≤1A |
| Energy Consumption： | <0.5W |
| Lifespan： | ≥ 100,000 times at 110V operating voltage |
| Installation Limitation： | It cannot be installed in a metal shield and magnetic interference place |
| Working Temperature： | -10℃ - 60℃ |
| Dimension: | 122mm\*74mm |
| Cover Material： | ABS Non-flammable material |
| Color： | Black/White/Golden |
| Transmission Frequency： | 2.4GHz |

**3、Operating Steps：**

**3.1、On/Off**

On：The light will become brighter gradually。

Off：Shut the light。

**3.2 Brightness Adjustment**

Brighter: Touch “Brighter”, the light will become bright gradually。

Dim: Touch “Dim”, the light will become dim gradually。

You can hold or touch the switch to control.

**Note:** 1. You should touch the switch quickly, no more than 0.5s.

2. Please make sure the connected lamps can be dimmed, common bulb can’t be dimmed.

3、Maybe there will be lamp flashing because of lamp load, please adjust it to the stable status.

4、Please don’t connect with multiple pieces lamps(Strip Light) to prevent over-voltage.

4、Customer Service and Warranty

Yantai Wiscloud Cloud Computing Co., Ltd provides the following national warranty coverage for iWiscloud smart dimmer switch:

1.If there is performance failure, customers can return, exchange or repair products within 7 days from the date of original retail purchase.

2.If there is performance failure, customers can exchange or repair products within 15 days from the date of original retail purchase.

3.12 months warranty covered from the date of original retail purchase, but the parts warranty are not covered.

4.iWiscloud Smart Dimmer Switch is warranted for the specified Warranty Period from the date of original retail purchase against defects in quality and materials under normal, non-commercial use. Abnormal usage caused damage is not warranty covered. Abnormal usage includes (force majeure), but limited to, deliberate damaging, disassembling, dismantle, manipulating warranty stick, power overloading, water damaging or other man-made caused product damages.

5、Product Checklist

|  |  |
| --- | --- |
| Items | Quantity |
| iWiscloud smart dimmer switch (US edition) | 1 |
| Instruction Manual | 1 |
| Fastening screws | 2 |
| Warranty Card | 1 |
| Quality Control Certificate | 1 |

6、Company Information

URL: <http://en.iwiscloud.com>

E-mail：[service@iwiscloud.com](mailto:service@iwiscloud.com)

**Yantai Wiscloud Cloud Computing Co., Ltd. reserves its right in the terms and conditions interpretation found within this operational manual.**